*GND -------------------------- GND*

GP2 -------------------------- Not connected (open)

GP0 -------------------------- GND

RXD -------------------------- RX

TXD -------------------------- TX

CHPD ------------------------ 3.3V

RST -------------------------- Not connected (open)

VCC -------------------------- 3.3V

